Karl Schmidt
Transtronics, Inc.

3209 W. 9th Street
Lawrence, KS 66049

(785) 841 3089
FAX (785) 841 0434
karl@xtronics.com
Web: http://xtronics.com

-PCB Name and revision number Memcal 1.0 - ron??
-We provide Gerber files including drill layer
  holes - two sizes - smaller 32 mil, larger 40 mil
-FR4 .062"
-Quantity 100
-Sides 2
-Silk Screen 1 (white or yellow)
-Solder Mask 2 sides green/matte finish SR1000 over bare copper (same art work)
-10 mil clearance and 15 mil features
-Size 3.475" X 1.7"  
-To IPC specifications
-Conductor widths and spacing shall be within +/- .001" of artwork originals.
-1 oz copper
-hole dimensions are finished size
-Use job name on negative to identify charges on invoice

FILES ---
README       = THIS FILE

.brd	= EAGLE PC board file
.sch	= EAGLE schematic file

Gerb274X.cam generated files:
.cmp	= Gerber component side
.gpi	= Gerber drill info
.plc	= Gerber silkscreen legend and board outline
.sol	= Gerber solder side
.stc	= Gerber solder mask, component side
.sts	= Gerber solder mask, solder side

Excellon.cam generated files:
.drd	= ?
.dri	= Excellon drill info